geometry_msgs/PoseStamped pose_stamped  # The robot's pose when the recovery was triggered
uint16 current_recovery_number          # 0-based index of current recovery number
uint16 total_number_of_recoveries       # Total number of recoveries configured
string recovery_behavior_name           # Namespace of the recovery being executed
